# Chapter 13. A Miscellany of Scripts

#### Contents:

uutot.awk--Report UUCP Statistics
phonebill--Track Phone Usage
combine--Extract Multipart uuencoded Binaries
mailavg--Check Size of Mailboxes
adj--Adjust Lines for Text Files
readsource--Format Program Source Files for troff
gent--Get a termcap Entry
plpr--lpr Preprocessor
transpose--Perform a Matrix Transposition
m1--Simple Macro Processor

This chapter contains a miscellany of scripts contributed by Usenet users. Each program is introduced with a brief description by the program's author. Our comments are placed inside brackets [like this]. Then the full program listing is shown. If the author did not supply an example, we generate one and describe it after the listing. Finally, in Section 13.1.1, we talk briefly about the program, highlighting some interesting points. Here is a summary of the scripts:

uutot.awk
  Report UUCP statistics.
phonebill
  Track phone usage.
combine
  Extract multipart uuencoded binaries.
mailavg
  Check size of mailboxes.
adj
  Adjust lines for text files.
readsource
  Format program source files for troff.
gent
  Get a termcap entry.
plpr
  lpr preprocessor.
transpose
  Perform a matrix transposition.
m1
  A very simple macro processor.

## 13.1. uutot.awk--Report UUCP Statistics

Contributed by Roger A. Cornelius

Here's something I wrote in nawk in response to all the C versions of the same thing which were posted to alt.sources awhile back. Basically, it summarizes statistics of uucp connections (connect time, throughput, files transmitted, etc.). It only supports HDB-style log files, but will show statistics on a site-by-site, or on an overall (all sites), basis. [It also works with /usr/spool/uucp/SYSLOG.]

I use a shell wrapper which calls "awk -f" to run this, but it's not necessary. Usage information is in the header. (Sorry about the lack of comments.)

>     # @(#) uutot.awk - display uucp statistics - requires new awk
>     # @(#) Usage:awk -f uutot.awk [site ...] /usr/spool/uucp/.Admin/xferstats
>     # Author: Roger A. Cornelius (rac@sherpa.uucp)

>     #       dosome[];               # site names to work for - all if not set
>     #       remote[];               # array of site names
>     #       bytes[];                # bytes xmitted by site
>     #       time[];	               # time spent by site
>     #       files[];                # files xmitted by site
>     BEGIN {
>     	doall = 1;
>     	if (ARGC > 2) {
>     		doall = 0;
>     		for (i = 1; i < ARGC-1; i++) {
>     			dosome[ ARGV[i] ];
>     			ARGV[i] = "";
>     		}
>     	}

>     	kbyte = 1024	# 1000 if you're not picky
>     	bang = "!";
>     	sending = "->";
>     	xmitting = "->" "|" "<-";

>     	hdr1 = "Remote     K-Bytes   K-Bytes   K-Bytes " \
>     		"Hr:Mn:Sc Hr:Mn:Sc AvCPS AvCPS    #    #\n";
>     	hdr2 = "SiteName      Recv      Xmit     Total     " \
>     		"Recv     Xmit  Recv  Xmit Recv Xmit\n";

>     	hdr3 = "-------- --------- --------- --------- -------- " \
>     		"-------- ----- ----- ---- ----";
>     	fmt1 = "%-8.8s %9.3f %9.3f %9.3f %2d:%02d:%02.0f " \
>     		"%2d:%02d:%02.0f %5.0f %5.0f %4d %4d\n";
>     	fmt2 = "Totals   %9.3f %9.3f %9.3f %2d:%02d:%02.0f " \
>     		"%2d:%02d:%02.0f %5.0f %5.0f %4d %4d\n";
>     }
>     {
>     	if ($6 !~ xmitting)		# should never be
>     		next;
>     	direction = ($6 == sending ? 1 : 2)

>     	site = substr($1,1,index($1,bang)-1);
>     	if (site in dosome || doall) {
>     		remote[site];
>     		bytes[site,direction] += $7;
>     		time[site,direction] += $9;
>     		files[site,direction]++;
>     	}
>     }
>     END {
>     	print hdr1 hdr2 hdr3;
>     	for (k in remote) {
>     		rbyte += bytes[k,2];	sbyte += bytes[k,1];
>     		rtime += time[k,2];	stime += time[k,1];
>     		rfiles += files[k,2];	sfiles += files[k,1];
>     		printf(fmt1, k, bytes[k,2]/kbyte, bytes[k,1]/kbyte,
>     			(bytes[k,2]+bytes[k,1])/kbyte,
>     			time[k,2]/3600, (time[k,2]%3600)/60, time[k,2]%60,
>     			time[k,1]/3600, (time[k,1]%3600)/60, time[k,1]%60,
>     			bytes[k,2] && time[k,2] ? bytes[k,2]/time[k,2] : 0,
>     			bytes[k,1] && time[k,1] ? bytes[k,1]/time[k,1] : 0,
>     			files[k,2], files[k,1]);
>     	}

>     	print hdr3
>     	printf(fmt2, rbyte/kbyte, sbyte/kbyte, (rbyte+sbyte)/kbyte,
>     		rtime/3600, (rtime%3600)/60, rtime%60,
>     		stime/3600, (stime%3600)/60, stime%60,
>     		rbyte && rtime ? rbyte/rtime : 0,
>     		sbyte && stime ? sbyte/stime : 0,
>     		rfiles, sfiles);
>     }

A test file was generated to test Cornelius' program. Here are a few lines extracted from /usr/spool/uucp/.Admin/xferstats (because each line in this file is too long to print on a page, we have broken the line following the directional arrow for display purposes only):

>     isla!nuucp S (8/3-16:10:17) (C,126,25) [ttyi1j] ->
>                          1131/4.880 secs, 231 bytes/sec
>     isla!nuucp S (8/3-16:10:20) (C,126,26) [ttyi1j] ->
>                          149/0.500 secs, 298 bytes/sec

>     isla!sue S (8/3-16:10:49) (C,126,27) [ttyi1j] ->
>                          646/25.230 secs, 25 bytes/sec
>     isla!sue S (8/3-16:10:52) (C,126,28) [ttyi1j] ->
>                          145/0.510 secs, 284 bytes/sec
>     uunet!uisla M (8/3-16:15:50) (C,951,1) [cui1a] ->
>                          1191/0.660 secs, 1804 bytes/sec
>     uunet!uisla M (8/3-16:15:53) (C,951,2) [cui1a] ->
>                          148/0.080 secs, 1850 bytes/sec
>     uunet!uisla M (8/3-16:15:57) (C,951,3) [cui1a] ->
>                          1018/0.550 secs, 1850 bytes/sec
>     uunet!uisla M (8/3-16:16:00) (C,951,4) [cui1a] ->
>                          160/0.070 secs, 2285 bytes/sec
>     uunet!daemon M (8/3-16:16:06) (C,951,5) [cui1a] <-
>                          552/2.740 secs, 201 bytes/sec
>     uunet!daemon M (8/3-16:16:09) (C,951,6) [cui1a] <-
>                          102/1.390 secs, 73 bytes/sec

Note that there are 12 fields; however, the program really only uses fields 1, 6, 7, and 9. Running the program on the sample input produces the following results:

>     $ nawk -f uutot.awk uutot.test
>     Remote     K-Bytes   K-Bytes   K-Bytes Hr:Mn:Sc Hr:Mn:Sc AvCPS AvCPS    #    #
>     SiteName      Recv      Xmit     Total     Recv     Xmit  Recv  Xmit Recv Xmit
>     -------- --------- --------- --------- -------- -------- ----- ----- ---- ----
>     uunet        0.639     2.458     3.097  0:04:34  2:09:49     2     0    2    4
>     isla         0.000     2.022     2.022  0:00:00  0:13:58     0     2    0    4
>     -------- --------- --------- --------- -------- -------- ----- ----- ---- ----
>     Totals       0.639     4.480     5.119  0:04:34  2:23:47     2     1    2    8

### 13.1.1. Program Notes for uutot.awk

This nawk application is an excellent example of a clearly written awk program. It is also a typical example of using awk to change a rather obscure UNIX log into a useful report.

Although Cornelius apologizes for the lack of comments that explain the logic of the program, the usage of the program is clear from the initial comments. Also, he uses variables to define search patterns and the report's layout. This helps to simplify conditional and print statements in the body of the program. It also helps that the variables have names which aid in immediately recognizing their purpose.

This program has a three-part structure, as we emphasized in Chapter 7, "Writing Scripts for awk". It consists of a BEGIN procedure, in which variables are defined; the body, in which each line of data from the log file is processed; and the END procedure, in which the output for the report is generated.

Copyright © 2003 O'Reilly & Associates. All rights reserved.